
Teams Rooms Accessories Compatibility Lists




 **TIP**

For a detailed introduction to each accessory and supported endpoints, please refer to [Meeting Room Endpoints Accessories](https://support.yealink.com/en/portal/knowledge/show?id=64b136b95b323b55e7a979ba).

Enabling the host Wi-Fi may affect the use of the wireless content-sharing dongle and the wireless microphone. For more information, refer to Can the Host Wi-Fi, Wireless Content Sharing Dongle, and the Wireless Microphone Be Enabled Simultaneously?

**MeetingBar Compatibility**



 **NOTE**


Different versions of the VCR20 cannot be mixed between MTRoW and MTRoA systems.

The microphones of different models in the list cannot be mixed; however, the VCM36-W is an expansion microphone that can be used with the built-in microphone.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **MeetingBar A10** | **MeetingBar A20** | **MeetingBar A30** | **MeetingBar A40** |
| WPP20 | × | Support pairing up to 4 but only using 1 at a time | Support pairing up to 4 but only using 1 at a time | × |
| WPP30 | Support pairing up to 4 but only using 1 at a time | Support pairing up to 4 but only using 1 at a time | Support pairing up to 4 but only using 1 at a time | Support pairing up to 4 but only using 1 at a time (Only for sharing) |
| PA20 | Support pairing up to 4 but only using 1 at a time (Only for sharing) | Support pairing up to 4 but only using 1 at a time (Only for sharing) | Support pairing up to 4 but only using 1 at a time (Only for sharing) | Support pairing up to 4 but only using 1 at a time (Only for sharing) |
| VCH51 | × | Support pairing up to 1 | Support pairing up to 1 | × |
| VCM34 | × | Support pairing/using up to 2 at a time | Support pairing/using up to 3 at a time | × |
| VCM35 | × | Support pairing/using up to 2 (A20 version requires 133.320.0.12 and later) | Support pairing/using up to 3 (A30 version requires 133.320.0.12 and later) | Support pairing/using up to 2 |
| VCM36-W | × | Support pairing/using up to 1 (A20 version requires 133.320.0.2 and later) | Support pairing/using up to 2 (A30 version requires 133.320.0.2 and later) | Support pairing/using up to 2 |
| VCM38 | × | Support pairing/using up to 2 at a time | Support pairing/using up to 3 at a time | × |
| CPW65 | × | × | × | × |
| CPW90-BT | × | × | × | × |
| CPW90 | × | Support pairing/using up to 1 pair (i.e., 2 CPW90 at a time) | Support pairing/using up to 1 pair (i.e., 2 CPW90 at a time) | × |
| CM20 | × | Coming soon | Coming soon | 2 (A40 version requires 289.320.0.31 and later) |
| CS10 | × | Coming soon | Coming soon | 2 (A40 version requires 289.320.0.31 and later) |
| CP50 | × | x | x | x |
| CPE40 | × | x | x | x |
| MSpeaker II | × | × | × | × |
| MSpeech | × | × | × | × |
| UVC30 | × | × | × | × |
| UVC84/UVC 86 | × | × | × | × |
| MB-CAM- 6X/12X | × | × | × | × |
| CTP18 | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | × |
| CTP25 | × | × | × | Support pairing/using up to 1 at a time |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| MTouch II/Plus/E2 | × | × | × | × |
| VCR11 | √ | √ | √ | √ |
| VCR20 | × | √ | √ | × |

**MeetingBoard 65/86 Compatibility**



 **NOTE**

The VCM35/VCM36-W is used as an expansion microphone.

|  |  |
| --- | --- |
| **Item** | **MeetingBoard 65&86** |
| WPP20 | Support pairing up to 4, using 1 at a time. |
| WPP30 | Support pairing up to 4, using 1 at a time.  (MeetingBoard 65&86 version requires 155.15.0.37 and later |
| PA20 | Support pairing up to 4 but only using 1 at a time (MeetingBoard version requires 155.15.0.37 and later) |
| VCH51 | Support pairing/using up to 1 at a time |
| VCM34 | × |
| VCM35 | Support pairing/using up to 2  (MeetingBoard 65&86 version requires 155.15.0.46 and later) |
| VCM36-W | Support pairing/using up to 2  (MeetingBoard 65&86 version requires 155.15.0.46 and later) |
| VCM38 | × |
| CPW90-BT | × |
| CPW90 | × |
| CPW65 | × |
| CP50 | × |
| CPE40 | × |
| CM20 | × |
| CS10 | × |
| MSpeaker II | × |
| MSpeech | × |
| UVC30 | × |
| UVC84 or UVC86 | Support pairing/using up to 1 (MeetingBoard 65&86 version requires 155.15.0.59 and later) |
| MB-CAM-6X/12X | MB-CAM-6X: Support pairing/using up to 1  (MeetingBoard 65&86 version requires 155.15.0.37 and later)  MB-CAM-12X: MeetingBoard 65&86 version requires 155.15.0.46 and later |
| MCore OPS | Support pairing/using up to 1  (MeetingBoard 65&86 version requires 155.15.0.37 and later) |
| CTP18 | Support pairing/using up to 1  (MeetingBoard 65&86 version requires 155.15.0.37 and later) |
| ETV65&86 | Support pairing/using up to 1  (MeetingBoard 65&86 version requires 155.15.0.46 and later) |
| RoomPanel&RoomPanel Plus | Support pairing/using up to 1  (MeetingBoard 65&86 version requires 155.15.0.46 and later) |
| MTouch II/Plus/E2 | × |
| VCR11 | × |
| VCR20 | × |

**MVC (MTR) Compatibility**

**Important Notes**

 **Additional Camera Limitations for MVC Kits:**

 **MVC Kit with AVHub:** Can connect up to 9 UVC Cameras. Refer to **Limitations on Yealink AVHub with UVC Cameras** below for further details.

 **MVC Kit without AVHub:** Can connect up to 1 UVC Camera.

 **Limitations on Yealink AVHub with UVC Cameras:**

 If connecting the UVC84/UVC86 directly to the AVHub, ensure the total connections do not exceed 2 UVC86 or 4 UVC84. If the connections exceed these limits, a PoE switch compliant with the 802.3 AT (PoE+) standard is required.

 When an AVHub is connected to a PoE switch, it supports connecting to up to 9 UVC Cameras.

 **Limitations on Yealink AVHub with CS10/CM20:**

 When connecting the CS10 to the AVHub, CS10 is compatible with VCM36-W, CPW65, VCM38, and VCM35 microphones.

 A single AVHub supports up to 2 CS10s and 2 CM20s, but connecting more than 3 speakers simultaneously is not recommended due to the risk of insufficient power

 **External Microphone Compatibility with MVC:**

 The following microphones are external and compatible with MVC devices: Yealink Array Microphone (VCM), Yealink DECT Wireless Mic (CPW), and Yealink Ceiling Microphone (CM).

 The MVC S40 supports VCM35/VCM36-W as expansion microphones and can work together with the built-in microphone of the MVC S40.  The MVC S40 supports CM20 as expansion microphones **but cannot work together with** the built-in microphone of the MVC S40.

 **CM20/CS10 Compatibility with MVC Packages (without AVHub):**

 CS10 is compatible only with CM20.

 CM20 is compatible only with CS10 and MSpeaker II.

 **Connect CM20/CS10 via a PoE Switch:**

 Ensure that the switch is a Gigabit Ethernet switch without the EEE feature (or the EEE feature can be disabled). For instance, the EEE feature of RCH40 cannot be disabled, so it cannot be connected to the CM20/CS10.

 For a single RCH40 E2, the power supply supports up to 2 CM20s and 2 CS10s, or 3 CS10s only. Connecting 4 speakers simultaneously should be avoided due to the risk of insufficient power.

**Microphone Priority for MVC Devices**

MVC devices do not support audio mixing for connected microphones. The audio input device with the highest priority will be used in the following order: **CM20 > VCM38 > VCM35 > VCM34 > VCM36-W > CPW90/CPW90-BT > CPW65 > Line-In > Built-in microphone > USB to Line-In**.

**MVC-3rd-Gen Device Compatibility**

**The devices are included in the combination product by default.**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **MVC340** | **MVC400** | **MVC640** | **MVC840** | **MVC860** |
| UVC34  MCore Pro MTouch E2 | UVC40  MCore Pro MTouch E2 | UVC84  MCore Pro MTouch E2 | MCore Pro UVC84  MTouch Plus RoomSensor | UVC86  MCore Pro MTouch Plus RoomSensor |

|  |  |  |  |
| --- | --- | --- | --- |
| **MVC940** | **MVCS60** | **MVCS40** | **MVCS90** |
| MCore Pro |  | MCore Pro MTouch E2 (C4) MTouch Plus (C5) RoomSensor (C5) SmartVision 40 | UVC86  MCore Pro MTouch Plus RoomSensor WPP30  MVC-BYOD-Extender AVHub |
| MTouch Plus | RoomSensor |
| AVHub | SmartVision 60 |
| RoomSensor | MTouch Plus |
| WPP30 | MCore Pro |
| UVC84 |  |

**The maximum number of accessories supported by the combination**

**Table 1:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item** | **MVC340** | **MVC400** | **MVC640** | **MVC840** | **MVC860** |
| WPP20 | × | × | × | × | × |
| WPP30 | √（Support pairing up to 8, connecting 4 but only using 1 at a time） | √（Support pairing up to 8, connecting 4 but only using 1 at a time） | √（Support pairing up to 8, connecting 4 but only using 1 at a time） | √（Support pairing up to 8, connecting 4 but only using 1 at a time） | √（Support pairing up to 8, connecting 4 but only using 1 at a time） |
| PA20 | Support pairing up to 8, connecting 4 but only using 1 at a time | Support pairing up to 8, connecting 4 but only using 1 at a time | Support pairing up to 8, connecting 4 but only using 1 at a time | Support pairing up to 8, connecting 4 but only using 1 at a time | Support pairing up to 8, connecting 4 but only using 1 at a time |
| VCH51 | × | × | × | × | × |
| VCM34 | × | √（Support pairing/using up to 2 at a time） | √（Support pairing/using up to 6 at a time） | √（Support pairing/using up to 6 at a time） | √（Support pairing/using up to 6 at a time） |
| VCM35 | × | × | √（Support pairing/using up to 8 at a time） | √（Support pairing/using up to 8 at a time） | √（Support pairing/using up to 8 at a time） |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| VCM36-W | × | × | √（Support pairing/using up to 2 at a time） | √（Support pairing/using up to 2 at a time） | √（Support pairing/using up to 4 at a time） |
| VCM38 | × | √（Support pairing/using up to 2 at a time） | √（Support pairing/using up to 8 at a time） | √（Support pairing/using up to 8 at a time） | √（Support pairing/using up to 8 at a time） |
| CPW65 | × | × | √（Support pairing/using up to 1 pair, i.e., 2 CPW65 at a time） | √（Support pairing/using up to 1 pair, i.e., 2 CPW65 at a time） | √（Support pairing/using up to 1 pair, i.e., 2 CPW65 at a time） |
| CPW90 | × | √（Support pairing/using up to 1 pair, i.e., 2 CPW90 at a time） | √（Support pairing/using up to 2 pairs, i.e., 4 CPW90 at a time） | √（Support pairing/using up to 2 pairs, i.e., 4 CPW90 at a time） | √（Support pairing/using up to 2 pairs, i.e., 4 CPW90 at a time） |
| CPW90-BT | × | × | × | × | × |
| CM20 | × | × | Support pairing/using up to 4 (Connect to UVC84 and its version requires 262.433.0.10 and later)  The Line Out port of the UVC84 will become unavailable | Support pairing/using up to 4 (Connect to UVC84 and its version requires 262.433.0.10 and later)  The Line Out port of the UVC84 will become unavailable | Support pairing/using up to 4 (Connect to UVC86 and its version requires 151.433.0.15 and later) |
| CS10 | × | × | Support pairing/using up to 4 (Connect to UVC84 and its version requires 262.433.0.10 and later)  Only work with CM20 | Support pairing/using up to 4 (Connect to UVC84 and its version requires 262.433.0.10 and later)  Only work with CM20 | Support pairing/using up to 4 (Connect to UVC86 and its version requires 151.433.0.15 and later)  Only work with CM20 |
| MSpeaker II | × | × | √（Support pairing/using up to 4 at a time） | √（Support pairing/using up to 4 at a time） | √（Support pairing/using up to 4 at a time） |
| MSpeech | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） |
| UVC30  Content Camera | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） |
| UVC84  /UVC86 | × | × | Support pairing/using up to 1 UVC84 | Support pairing/using up to 1 UVC84 | Support pairing/using up to 1 UVC86 |
| MB-CAM- 6X/12X | × | × | × | × | × |
| CTP18 | × | × | × | × | × |
| MTouch (E2/Plus) | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） |
| RoomSenso r | × | × | × | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） |
| VCR11 | × | × | × | × | × |
| VCR20 | √ | √ | √ | √ | √ |
| MVC-BYOD-  Extender | × | √ | √ | √ | √ |

**Table 2:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **MVC940** | **MVCS60** | **MVCS40** | **MVCS90** |
| WPP20 | × | × | × | × |
| WPP30 | √（Support pairing up to 8, connecting 4 but only using 1 at a time） | √（Support pairing up to 8, connecting 4 but only using 1 at a time, do not support BYOD） | √（Support pairing up to 8, connecting 4 but only using 1 at a time） | √（Support pairing up to 8, connecting 4 but only using 1 at a time） |
| PA20 | Support pairing up to 8, connecting 4 but only using 1 at a time | Support pairing up to 8, connecting 4 but only using 1 at a time | Support pairing up to 8, connecting 4 but only using 1 at a time | Support pairing up to 8, connecting 4 but only using 1 at a time |
| VCH51 | × | × | × | × |
| VCM34 | √（Support pairing/using up to 8 at a time） | × | × | √（Support pairing/using up to 8 at a time） |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| VCM35 | √（Support pairing/using up to 8 at a time） | × | √（Support pairing/using up to 2 at a time） | √（Support pairing/using up to 8 at a time） |
| VCM36-W | × | × | √ （Support pairing/using up to 2 at a time） | × |
| VCM38 | √（Support pairing/using up to 8 at a time） | × | × | √（Support pairing/using up to 8 at a time） |
| CPW65 | √（Support pairing/using up to 1 pair, i.e., 2 CPW65 at a time） | × | × | √（Support pairing/using up to 1 pair, i.e., 2 CPW65 at a time） |
| CPW90 | √（Support pairing/using up to 2 pairs, i.e., 4 CPW90 at a time） | × | × | √（Support pairing/using up to 2 pair, i.e., 4 CPW90 at a time） |
| CPW90-BT | × | × | × | × |
| CM20 | Support pairing/using up to 4 (Connect to AVHub and its version requires 153.433.0.15 and later) | × | √（Support pairing/using up to 2 at a time） | Support pairing/using up to 4 (Connect to AVHub and its version requires 153.433.0.15 and later) |
| CS10 | Support pairing/using up to 4 (Connect to AVHub and its version requires 153.433.0.15 and later) | × | √（Support pairing/using up to 2 at a time） | Support pairing/using up to 4 (Connect to AVHub and its version requires 153.433.0.15 and later) |
| MSpeaker II | √（Support pairing/using up to 4 at a time） | × | × | √（Support pairing/using up to 4 at a time） |
| MSpeech | √（Support pairing/using up to 1 at a time） | × | × | √（Support pairing/using up to 1 at a time） |
| UVC30  Content Camera | √（Support pairing/using up to 1 at a time） | × | √ Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） |
| UVC84  /UVC86 | √（Support pairing/using up to 9 at a time） | × | × | √（Support pairing/using up to 9 at a time） |
| MB-CAM- 6X/12X | × | × | × | × |
| CTP18 | × | × | × | × |
| MTouch (E2/Plus) | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） |
| RoomSenso r | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） | √（Support pairing/using up to 1 at a time） |
| VCR11 | × | × | √ | × |
| VCR20 | √ | × | √ | √ |
| MVC-BYOD-  Extender | √ | × | √ | √ |

**MVC-2nd-Gen Device Compatibility**

**The devices are included in the combination product by default.**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **MVC320** | **MVC400** | **MVC640** | **MVC640-Wireless** | **MVC660** | **MVC840** | **MVC840-Base Kit** |
| * MCore * MTouch II * UVC30 * MSpeech | MCore MTouch II UVC40 | * MCore Pro * MTouch II * UVC84 * MSpeech * WPP20 (optional) | * MCore Pro * MTouch II * UVC84 * MSPeakerⅡ * CPW90 * WPP20(optional) | * MCore Pro * MTouch II * UVC86 * MSpeech * WPP20 (optional) | * MCore Pro * MTouch II * UVC84 * MSpeaker Ⅱ（optional） * WPP20 (optional) * VCM34（optional） * RCH40（optional） | * MCore Pro * MTouch II * UVC84 * MSpeaker Ⅱ（optional） * WPP20 (optional) * RCH40（optional） |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **MVC860** | **MVC860-Base Kit** | **MVC900** | **MVC940** | **MVC960** |
| * MCore Pro * MTouch II * UVC86 * VCM34 (optional) * VCM38 (optional) * RCH40 (optional) * MSpeaker Ⅱ (optional) * WPP20 (optional) * CPW90 (optional) | * MCore Pro * MTouch II * UVC86 * VCM38 (optional) * RCH40 (optional) * MSpeaker Ⅱ (optional) * WPP20 (optional) * CPW90 (optional) | * MCore Pro * MTouch Plus * AVHub * RoomSensor * MVC-BYOD-Extender | * MCore Pro * UVC84 * MTouch II * AVHub * WPP20 | * MCore Pro * MTouch II * UVC86 * VCM34 (optional) * VCM38 (optional) * CPW90 (optional) * MSpeaker Ⅱ (optional) * WPP20 (optional) * AVHub |

**The maximum number of accessories supported by the combination**

:::

**Table 1:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Item** | **MVC960** | **MVC940** | **MVC900** | **MVC860-BASE KIT[1]** | **MVC860[1]** | **MVC840-BASE KIT[1]** |
| WPP20 | Support pairing up to 8 but only using 1 at a time | Support pairing up to 8 but only using 1 at a time | Support pairing up to 8 but only using 1 at a time | Support pairing up to 8 but only using 1 at a time | Support pairing up to 8 but only using 1 at a time | Support pairing up to 8 but only using 1 at a time |
| WPP30 | Not compatible with MTouch II; compatible with MTouch E2 and MTouch Plus | Not compatible with MTouch II; compatible with MTouch E2 and MTouch Plus | Not compatible with MTouch II; compatible with MTouch E2 and MTouch Plus | Not compatible with MTouch II; compatible with MTouch E2 and MTouch Plus | Not compatible with MTouch II; compatible with MTouch E2 and MTouch Plus | Not compatible with MTouch II; compatible with MTouch E2 and MTouch Plus |
| PA20 | x | x | x | x | x | x |
| VCH51 | × | × | × | × | × | × |
| VCM34 | Support pairing/using up to 8 at a time | Support pairing/using up to 8 at a time | Support pairing/using up to 8 at a time | Support pairing/using up to 6 at a time | Support pairing/using up to 6 at a time | Support pairing/using up to 6 at a time |
| VCM35 | Support pairing/using up to 8 at a time (Connect to AVHub and its version requires 153.431.0.5 and later) | Support pairing/using up to 8 at a time (Connect to AVHub and its version requires 153.431.0.5 and later) | Support pairing/using up to 8 at a time (Connect to AVHub and its version requires 153.431.0.5 and later) | Support pairing/using up to 8 at a time (Connect to UVC86 and its version requires 151.431.0.5 and later) | Support pairing/using up to 8 at a time (Connect to UVC86 and its version requires 151.431.0.5 and later) | Support pairing/using up to 8 at a time (Connect to UVC84 and its version requires 262.431.0.5 and later) |
| VCM36-W | × | × | × | Support pairing/using up to 4 at a time (Connect to UVC86 and its version requires 151.431.0.5 and later) | Support pairing/using up to 4 at a time (Connect to UVC86 and its version requires 151.431.0.5 and later) | Support pairing/using up to 2 at a time (Connect to UVC84 and its version requires 262.431.0.5 and later) |
| VCM38 | Support pairing/using up to 8 at a time | Support pairing/using up to 8 at a time | Support pairing/using up to 8 at a time | Support pairing/using up to 8 at a time | Support pairing/using up to 8 at a time | Support pairing/using up to 8 at a time |
| CPW90-BT | × | × | × | × | × | × |
| CPW90 | Support pairing/using up to 2 pairs, i.e., 4 CPW90 at a time | Support pairing/using up to 2 pairs, i.e., 4 CPW90 at a time | Support pairing/using up to 2 pairs, i.e., 4 CPW90 at a time | Support pairing/using up to 2 pairs, i.e., 4 CPW90 at a time | Support pairing/using up to 2 pairs, i.e., 4 CPW90 at a time | Support pairing/using up to 2 pairs, i.e., 4 CPW90 at a time |
| CPW65 | Support pairing/using up to 2 (Connect to AVHub and its version requires 153.431.0.5 and later) | Support pairing/using up to 2 (Connect to AVHub and its version requires 153.431.0.5 and later) | Support pairing/using up to 2 (Connect to AVHub and its version requires 153.431.0.5 and later) | Support pairing/using up to 2 (Connect to UVC86 and its version requires 151.431.0.5 and later) | Support pairing/using up to 2 (Connect to UVC86 and its version requires 151.431.0.5 and later) | Support pairing/using up to 2 (Connect to UVC84 and its version requires 262.431.0.5 and later) |
| CM20 | Support pairing/using up to 4 (Connect to AVHub and its version requires 153.433.0.15 and later) | Support pairing/using up to 4 (Connect to AVHub and its version requires 153.433.0.15 and later) | Support pairing/using up to 4 (Connect to AVHub and its version requires 153.433.0.15 and later) | Support pairing/using up to 4 (Connect to UVC86 and its version requires 151.433.0.15 and later) | Support pairing/using up to 4 (Connect to UVC86 and its version requires 151.433.0.15 and later) | Support pairing/using up to 4 (Connect to UVC84 and its version requires 262.433.0.10 and  later).  The Line Out port of the UVC84 will become unavailable. |
| CS10 | Support pairing/using up to 4 (Connect to AVHub and its version requires 153.433.0.15 and later) | Support pairing/using up to 4 (Connect to AVHub and its version requires 153.433.0.15 and later) | Support pairing/using up to 4 (Connect to AVHub and its version requires 153.433.0.15 and later) | Support pairing/using up to 4 (Connect to UVC86 and its version requires 151.433.0.15 and  later)  Only work with CM20 | Support pairing/using up to 4 (Connect to UVC86 and its version requires 151.433.0.15 and  later)  Only work with CM20 | Support pairing/using up to 4 (Connect to UVC84 and its version requires 262.433.0.10 and  later)  Only work with CM20 |
| MSpeaker II | Support pairing/using up to 4 at a time | Support pairing/using up to 4 at a time | Support pairing/using up to 4 at a time | Support pairing/using up to 4 at a time | Support pairing/using up to 4 at a time | Support pairing/using up to 4 at a time |
| MSpeech | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | × | Support pairing/using up to 1 at a time |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| UVC30 | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time |
| UVC84/UVC 86/UVC80 | Support pairing/using up to 9 at a time | Support pairing/using up to 9 at a time | Support pairing/using up to 9 at a time | Support pairing/using up to 9 at a time | Support pairing/using up to 9 at a time | Support pairing/using up to 9 at a time |
| MB-CAM- 6X/12X | × | × | × | × | × | × |
| CTP18 | × | × | × | × | × | × |
| MTouch II | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time |
| VCR11 | × | × | × | × | × | × |
| VCR20 | √ | √ | √ | √ | √ | √ |
| MVC-BYOD-  Extender | √ | √ | √ | √ | √ | √ |

**Table 2**:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Item** | **MVC840[1]** | **MVC660** | **MVC640-Wireless** | **MVC640-AI** | **MVC400** | **MVC320** |
| WPP20 | Support pairing up to 8 but only using 1 at a time | Support pairing up to 8 but only using 1 at a time | Support pairing up to 8 but only using 1 at a time | Support pairing up to 8 but only using 1 at a time | Support pairing up to 8 but only using 1 at a time | Support pairing up to 8 but only using 1 at a time |
| WPP30 | Not compatible with MTouch II; compatible with MTouch E2 and MTouch Plus | Not compatible with MTouch II; compatible with MTouch E2 and MTouch Plus | Not compatible with MTouch II; compatible with MTouch E2 and MTouch Plus | Not compatible with MTouch II; compatible with MTouch E2 and MTouch Plus | Not compatible with MTouch II; compatible with MTouch E2 and MTouch Plus | Not compatible with MTouch II; compatible with MTouch E2 and MTouch Plus |
| PA20 | x | x | x | x | x | x |
| VCH51 | × | × | × | × | × | × |
| VCM34 | Support pairing/using up to 6 at a time | × | × | × | Support pairing/using up to 2 at a time | × |
| VCM35 | Support pairing/using up to 8 at a time(Connect to UVC84 and its version requires 262.431.0.5 and later) | × | × | × | × | × |
| VCM36-W | Support pairing/using up to 2 at a time(Connect to UVC84 and its version requires 262.431.0.5 and later) | × | Support pairing/using up to 2 at a time (Connect to UVC84 and its version requires 262.431.0.5) | × | × | × |
| VCM38 | Support pairing/using up to 8 at a time | × | × | × | Support pairing/using up to 2 at a time | × |
| CPW90-BT | × | × | × | × | × | × |
| CPW90 | Support pairing/using up to 2 pairs, i.e., 4 CPW90 at a time | × | × | × | Support pairing/using up to 1 pair, i.e., 2 CPW90 at a time | × |
| CPW65 | Support pairing/using up to 2(Connect to UVC84 and its version requires 262.431.0.5 and later) | × | × | × | × | × |


|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| CM20 | Support pairing/using up to 4 (Connect to UVC84 and its version requires 262.433.0.10 and  later).  The Line Out port of the UVC84 will become unavailable. | Support pairing/using up to 4 (Connect to UVC86 and its version requires 151.433.0.15 and later) | Support pairing/using up to 4 (Connect to UVC84 and its version requires 262.433.0.10 and  later).  The Line Out port of the UVC84 will become unavailable. | Support pairing/using up to 4 (Connect to UVC84 and its version requires 262.433.0.10 and  later).  The Line Out port of the UVC84 will become unavailable. | × | × |
| CS10 | Support pairing/using up to 4 (Connect to UVC84 and its version requires 262.433.0.10 and  later)  Only work with CM20 | Support pairing/using up to 4 (Connect to UVC86 and its version requires 151.433.0.15 and  later)  Only work with CM20 | Support pairing/using up to 4 (Connect to UVC84 and its version requires 262.433.0.10 and  later)  Only work with CM20 | Support pairing/using up to 4 (Connect to UVC84 and its version requires 262.433.0.10 and  later)  Only work with CM20 | × | × |
| MSpeaker II | Support pairing/using up to 4 at a time | × | Support pairing/using up to 4 at a time | × | × | × |
| MSpeech | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | × | Support pairing/using up to 1 at a time | × | Support pairing/using up to 1 at a time |
| UVC30 | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time |
| UVC84/UVC 86/UVC80 | × | × | × | × | × | × |
| MB-CAM- 6X/12X | × | × | × | × | × | × |
| CTP18 | × | × | × | × | × | × |
| MTouch II | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time | Support pairing/using up to 1 at a time |
| VCR11 | × | × | × | × | × | × |
| VCR20 | √ | √ | √ | √ | √ | √ |
| MVC-BYOD-  Extender | √ | √ | √ | √ | √ | × |

**UVC Camera/AVHub Device Compatibility**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Item** | **SmartVisio n 40** | **AVHub** | **UVC86** | **UVC84** | **UVC40 E2** | **UVC40** | **UVC34** | **UVC30** | **UVC80** | **UVC50** |
| VCM34 | × | Support pairing/usin g up to 8 at a time | Support pairing/usin g up to 6 at a time | Support pairing/usin g up to 6 at a time | × | Support pairing/usin g up to 2 at a time | × | × | Support pairing/usin g up to 6 at a time | Support pairing/usin g up to 6 at a time |
| VCM35 | Support pairing/usin g up to 2 at a time | Support pairing/usin g up to 8 at a time (AVHub version requires 153.431.0.5  and later) | Support pairing/usin g up to 8 at a time (UVC86  version requires 151.431.0.5  and later) | Support pairing/usin g up to 8 at a time (UVC84  version requires 262.431.0.5  and later) | √ | × | × | × | × | × |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| VCM36-W | Support pairing/usin g up to 2 at a time | Support pairing/usin g up to 4 at a time (But the stability will be affected when AVHub is deployed inside the cabinet). | Support pairing/usin g up to 4 at a time (UVC86  version requires 151.431.0.5  and later) | Support pairing/usin g up to 2 at a time (UVC84  version requires 262.431.0.5  and later) | √ | × | × | × | × | × |
| VCM38 | × | Support pairing/usin g up to 8 at a time | Support pairing/usin g up to 8 at a time | Support pairing/usin g up to 8 at a time | × | Support pairing/usin g up to 2 at a time | × | × | Support pairing/usin g up to 6 at a time | Support pairing/usin g up to 6 at a time |
| CPW90-BT | × | × | × | × | × | × | × | × | Support pairing/usin g up to 2 pairs, i.e., 4 at a time | Support pairing/usin g up to 2 pairs, i.e., 4 at a time |
| CPW90 | × | Support pairing/usin g up to 2 pair, i.e., 4 at a time | Support pairing/usin g up to 2 pair, i.e., 4 at a time | Support pairing/usin g up to 1 pair, i.e., 2 at a time | × | Support pairing/usin g up to 1 pair, i.e., 2 at a time | × | Support pairing/usin g up to 2 pair, i.e., 4 at a time | × |  |
| CPW65 | × | Support pairing/usin g up to 1 pair, i.e., 2 (AVHub version requires 153.431.0.5  and later) | Support pairing/usin g up to 1 pair, i.e., 2 (UVC86  version requires 151.431.0.5  and later) | Support pairing/usin g up to 1 pair, i.e., 2 (UVC84  version requires 262.431.0.5  and later) | × | × | × | × | × | × |
| CM20 | Support pairing/usin g up to 2 at a time | Support pairing/usin g up to 4 (AVHub version requires 153.433.0.1  5 and later) | Support pairing/usin g up to 4 (UVC86  version requires 151.433.0.1  5 and later) | Suppor t pairing/ using up to 4 (Conne ct to UVC84  and its version require s 262.433  .0.10  and later). The Line  Out port of the UVC84  will become unavail able. | × | × | × | × | × | × |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| CS10 | Support pairing/usin g up to 2 at a time | Support pairing/usin g up to 4 (AVHub version requires 153.433.0.1  5 and later) | Suppor t pairing/ using up to 4 (Conne ct to UVC86  and its version require s 151.433  .0.15  and later) Only work  with CM20 | Suppor t pairing/ using up to 4 (Conne ct to UVC84  and its version require s 262.433  .0.10  and later) Only work  with CM20 | × | × | × | × | × | × |
| MSpeaker II | × | Support pairing/usin g up to 4 at a time | Support pairing/usin g up to 4 at a time | Support pairing/usin g up to 4 at a time | × | × | × | × | × | × |
| VCH51 | √ | x | x | x | x | x | x | x | x | x |
| VCR20 | √ | √ | √ | √ | √ | √ | √ | √ | √ | √ |
| MVC-BYOD-  Extender | √ | √ | √ | √ | × | √ | × | × | × | × |
| USB  Connector | √ | √ | √ | √ | √ | √ | √ | √ | √ | √ |



 **NOTE**

Different versions of the VCR20 remote control can control different devices. For more information, please refer to [VCR20 Remote Control Compatibility](https://support.yealink.com/en/portal/knowledge/show?id=624131b7c61a02257a68df42).

**DeskVision A24 Compatibility**

Wireless keyboard and mouse:

|  |  |
| --- | --- |
| **Brand** | **Model** |
| Logitech | K380 |
|  | K580 |
|  | K780 |
|  | MK270 |
| Surface Keyboard | Holgate |
|  | Surface Keyboard |
| HP | CS750 |
| lenovo | LBK500 |
|  | S6000 |
| PHILIPS | SPK6614 |
| RAPOO | XK100 |
| Acer | LK-416B |
| Apple | Magic Keyboard & Magic Mouse |

Headsets:

|  |  |  |
| --- | --- | --- |
| **Brand** | **Model** | **Connection Type** |
| Yealink | UH34/UH36/UH37/UH38 | USB |
| WH62/WH63/WH66/WH67 |
| Poly | Blackwire 3220 |
| Blackwire 3310 |
|  |

|  |  |  |
| --- | --- | --- |
|  | Blackwire 5220 |  |
| Jabra | Jabra Evolve 20 |
| Jabra Evolve 40 |
| Engage 65 Stereo & Mono |
| Engage 75 Stereo & Mono |
| Yealink | BH71/BH72/BH76 | Bluetooth |
| Poly | Voyager 4320 |
| Voyager Focus2 UC |
| Voyager Focus |
| VOYAGER 5200 |
| Legend |
| Jabra | Evolve 65 |
| Evolve 75 |
| Evolve2 65 |
| Evolve2 75 |
| Apple | AirPods |
| AirPods Pro |

**FAQ**

[**Can the built-in microphone and external microphone pick up sound at the same time?**](https://support.yealink.com/en/portal/knowledge/show?id=642bf9c18147a71021d9af99)

[**Does the MeetingBar AX0 support the simultaneous use of multiple microphone devices?**](https://support.yealink.com/en/portal/knowledge/show?id=642bdf848147a71021d9af36)

**Can the host Wi-Fi, wireless content sharing dongle, and the wireless microphone be enabled simultaneously?**

When the host Wi-Fi, wireless content sharing dongle, and the wireless microphone are simultaneously enabled, the compatibility is as follows:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Wireless Content Sharing Dongle is used** | **A10** | **A20** | **A30** | **A40** | **MeetingBoard 65/86** |
| Wireless Microphone | √ | √ | √ | √ | √ |
| Host Wi-Fi | × | × | × | √ | √ |
| **Host Wi-Fi is enabled** | **A10** | **A20** | **A30** | **A40** | **MeetingBoard 65/86** |
| Wireless Microphone | × | × | × | √ | √ |
| Wireless Content Sharing Dongle | × | × | × | √ | √ |
| **Wireless Microphone is used** | **A10** | **A20** | **A30** | **A40** | **MeetingBoard 65/86** |
| Host Wi-Fi | × | × | × | √ | √ |
| Wireless Content Sharing Dongle | √ | √ | √ | √ | √ |